                <li>Y. Song, <b><u>Y. Xu</u></b>, H. Ismail, X. Liu<sup>\*</sup>. Scour modeling based on immersed boundary method: A pathway to practical use of three-dimensional scour models, <i>Coastal Engineering</i>,2022:104037.

                </li>

                <li> Y.G. Lai<sup>\*</sup>, D. Smith, D. Bandrowski, <b><u>Y. Xu</u></b>, C. Woodley, K. Schnell. Development of a CFD model and procedure for flows through in-stream structures, <i>Journal of Applied Water Engineering and Research</i>,2021.

                </li>

<li> X. Hui, H. Yan<sup>\*</sup>, <b><u>Y. Xu</u></b>, H. Tan. Sprinkler droplet impact angle affects shear stress distribution on soil surface - A case study of a ball-driven sprinkler, <i>*Water Science and Technology: Water Supply*</i>, 2021, 21(6): 2772-2785.

</li>

<li> <b><u>Y. Xu</u></b> and X. Liu<sup>\*</sup>. An immersed boundary method with y+-adaptive wall function for smooth wall shear, <i>*International Journal for Numerical Methods in Fluids*</i>, 2021, 93:1929–1946.

</li>

<li> H. Ismail, <b><u>Y. Xu</u></b>, and X. Liu<sup>\*</sup>. Flow and Scour around Idealized Porous Engineered Log Jam Structures, <i>*Journal of Hydraulic Engineering*</i>, 2021, 147(1): 04020089.

</li>

<li>郑裕东，<b><u>**徐云成**</u></b>，严海军<sup>\*</sup>，郑永军. 基于近地遥感系统的小麦玉米冠层RVI和NDVI获取影响因素分析，<i>光谱学与光谱分析</i>，2021，41(8): 2578-2585.

</li>

<li>汪小珊，严海军，周凌九，<b><u>**徐云成**</u></b><sup>\*</sup>. SSQ系列射流施肥器水力性能试验研究，<i>农业工程学报</i>，2020，36(21): 31-38.

</li>

<li> Y. Song, <b><u>Y. Xu</u></b>, and X. Liu<sup>\*</sup>. Physically Based Sand Slide Method in Scour Models Based on Slope-Limited Diffusion, <i>*Journal of Hydraulic Engineering*</i>, 2020, 146(11): 4020074.

</li>

<li> H. Yan<sup>\*</sup>, X. Hui, M. Li, and <b><u>Y. Xu</u></b>. Development in sprinkler irrigation technology in China, <i>*Irrigation and Drainage*</i>, 2020, 69(S2): 75-87.

</li>

<li> <b><u>Y. Xu</u></b>, and X. Liu<sup>\*</sup>. Effects of Different In-Stream Structure Representations in Computational Fluid Dynamics Models—Taking Engineered Log Jams (ELJ) as an Example, <i>*Water*</i>, 2017, 9(2): 110.

</li>

<li> <b><u>Y. Xu</u></b>, and H. Yan<sup>\*</sup>. Numerical Simulation of Erosive Wear on an Impact Sprinkler Nozzle Using a Remeshing Algorithm, <i>*International Journal of Fluid Machinery and Systems*</i>, 2016, 9(4): 287-299.

</li>

<li> <b><u>Y. Xu</u></b>, Y. Chen, Z. Wang, L. Zhou, and H. Yan<sup>\*</sup>. Investigation of the cavitation fluctuation characteristics in a Venturi injector, <i>*Fluid Dynamics Research*</i>, 2015, 47(2): 025506.

</li>

<li> <b><u>Y. Xu</u></b>, Y. Chen, J. He, and H. Yan<sup>\*</sup>. Detection of cavitation in a Venturi injector with a combined method of strain gauges and numerical simulation, <i>*Journal of Fluids Engineering*</i>, 2014, 136(8): 081302.

</li>